#
PID/DATA MONITOR INSPECTION [JA5AX-EL]

id050206805600

1. Connect the WDS or equivalent to the DLC-2.

2. Turn the ignition switch to ON.

3. Measure the PID value.

  Note

  • Perform part inspection for the output device after TCM inspection.
  • The PID/DATA MONITOR function monitors the calculated value of the input/output signals in the TCM. Therefore, if a monitored value of an output device is out of specification, it is necessary to inspect the monitored value of the input device related to the output device control. Since an output device malfunction is not directly indicated as a malfunction of the monitored value for the output device, it is necessary to inspect the output device individually using the simulation function, etc.

PID/DATA MONITOR AND RECORD function table

Monitor item (Definition) | Unit/Condition | Condition/Specification | Action | TCM terminal
--- | --- | --- | --- | ---
24B_Duty (2-4 brake solenoid vale) | % | N position: 100 % M range (1GR) stall: 0 % | Inspect the 2-4 brake solenoid valve. (See SOLENOID VALVE INSPECTION [JA5AX-EL].) | 2V
BOO_TCM (Brake switch) | On/Off | Brake pedal depressed: ON Other: Off | Inspect the brake switch. (See BRAKE SWITCH INSPECTION.) | 1U
DTCCNT (Number of DTC detected) | - | DTCs is detected: 1-255 No DTCs are detected: 0 | Perform applicable DTC troubleshooting. (See DTC TABLE [JA5AX-EL].) | -
DWN_SW (Down switch) | On/Off | Down sift at M range: On Other: Off | Inspect the selector lever component. (See SELECTOR LEVER COMPONENT INSPECTION.) | 1S
ECT TCM (ECT sensor) | °C | Indicates engine coolant temperature | Inspect the ECT sensor. (See ENGINE COOLANT TEMPERATURE (ECT) SENSOR INSPECTION [L8, LF, L3].) Inspect the PCM (See PCM INSPECTION [L8, LF, L3].) | -
FDPDTC | - | Pending code that caused FFD storage | - | -
GEAR_SEL (Calculated gear range in TCM) | 1st/2nd/3rd/4th/5th | 1GR: 1st 2GR: 2nd 3GR: 3rd 4GR: 4th 5GR: 5th | Inspect following PIDs: THOP, TSS | -
HC_Duty (High clutch solenoid valve) | % | N position: 0 % D range 1GR to 2GR shifting: 100 % | Inspect the high clutch solenoid valve. (See SOLENOID VALVE INSPECTION [JA5AX-EL].) | 2U
LPS (Pressure control solenoid) | % | Ignition switch ON: 0% Idle: 0-100% | Inspect the pressure control solenoid. (See SOLENOID VALVE INSPECTION [JA5AX-EL].) | 2Y
MNL_SW (M range switch) | On/Off | M range: On Other: Off | Inspect the selector lever component. (See SELECTOR LEVER COMPONENT INSPECTION.) | 1AA
OSS (Intermediate sensor | RPM | Ignition switch ON: 0 RPM Idle: 700-800 RPM | Inspect the intermediate sensor. (See INTERMEDIATE SENSOR INSPECTION [JA5AX-EL].) | 1K, 1X
RPM_TCM (Engine speed) | RPM | Ignition switch ON: 0 RPM Idle: 700-800 RPM | Inspect the TCM. (See TCM INSPECTION [JA5AX-EL].) | -
SSA/SS1 (Shift solenoid A) | On/Off | N position: On D range 3GR: Off | Inspect the shift solenoid A. (See SOLENOID VALVE INSPECTION [JA5AX-EL].) | 2W
SSB/SS2 (Shift solenoid B) | On/Off | N position: On D range 4GR: Off | Inspect the shift solenoid B. (See SOLENOID VALVE INSPECTION [JA5AX-EL].) | 2T
SSC/SS3 (Shift solenoid C) | On/Off | N position: On D range 2GR: Off | Inspect the shift solenoid C. (See SOLENOID VALVE INSPECTION [JA5AX-EL].) | 2X
TCCC (TCC solenoid valve) | % | TCC operating: 100 % TCC non operating: 0 % | Inspect the TCC solenoid valve. (See SOLENOID VALVE INSPECTION [JA5AX-EL].) | 2S
TFT (ATF temperature) | °C | ATF 20 °C {68 °F}: 20 °C {68 °F} ATF 60 °C {140 °F}: 60 °C {140 °F} | Inspect the TFT sensor. (See TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR INSPECTION [JA5AX-EL].) | 1B, 1F
THOP (Throttle position) | % | CTP:0 % WOT: 100 % | Inspect the TCM. (See TCM INSPECTION [JA5AX-EL].) | -
TR (TR switch) | R/N/D | R position: R N position: N D range: D | Inspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5AX-EL].) | 1T, 1W, 1Z
TRD (TR switch [D range]) | On/Off | D range: On Other ranges and all positions: Off | Inspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5AX-EL].) | 1Z
TRR (TR switch [R position]) | On/Off | R position: On Other positions and all ranges: Off | Inspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5AX-EL].) | 1W
TSS (Input/turbine speed sensor) | RPM | Ignition switch ON: 0 RPM Idle: 700-800 RPM | Inspect the input/turbine speed sensor. (See INPUT/TURBINE SPEED SENSOR INSPECTION [JA5AX-EL].) | 1N, 2F
UP_SW (Up switch) | On/Off | Up sift at M range: On Other: Off | Inspect the selector lever component. (See SELECTOR LEVER COMPONENT INSPECTION.) | 2C
VPWR_TCM (Battery voltage) | V | IG ON: B+ Idle: 13-14 V | Inspect the main relay. (See RELAY INSPECTION.) | 1P
VSS (Vehicle speed) | KPH | Vehicle speed 20 km/h {12.5 mph}: 20 KPH Vehicle speed 40 km/h {25 mph}: 40 KPH | Inspect the vehicle speedometer sensor. (See VEHICLE SPEEDOMETER SENSOR (VSS) INSPECTION [JA5AX-EL].) | 1V, 1M