#
AIR MIX ACTUATOR REMOVAL/INSTALLATION

id074000802400

1. Disconnect the negative battery cable.

2. Remove the dashboard. (L.H.D.) (See DASHBOARD REMOVAL/INSTALLATION.)

3. Remove the glove compartment. (R.H.D.)

4. Remove the car navigation unit. (R.H.D.) (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)

5. Remove the blower motor. (L.H.D.) (See BLOWER MOTOR REMOVAL/INSTALLATION.)

6. Remove the resistor. (L.H.D.) (See RESISTOR REMOVAL/INSTALLATION.)

7. Remove the blower unit nuts. (L.H.D.)

8. Remove the screw securing the duct (2) to the A/C unit, by inserting a Phillips screwdriver into the hole made after removing the blower motor. (L.H.D.)

9. Remove the screw securing the duct (2) to the A/C unit. (L.H.D.)

10. Remove the duct (2). (L.H.D.)

11. Remove in the order indicated in the table.

L.H.D.

R.H.D.

1 | Air mix actuator connector
2 | Air mix actuator

12. Install in the duct (2). (L.H.D.)

13. Install the two outer screws, securing the duct (2) to the A/C unit. (L.H.D.)

14. Install the screw on the end of the Phillips screwdriver with the packing tape. (L.H.D.)

  Caution

  • If the packing tape remains in the duct (2), it may become a source of noise. Wind up the packing tape to prevent pinching when tightening the screw.

15. Install the duct (2) to the A//C unit by inserting a Phillips screwdriver, with the screw, into the hole made after removing the blower motor.

16. Pull out the Phillips screwdriver together with the packing tape.

17. Install the blower unit nuts. (L.H.D.)

18. Install the resistor. (L.H.D.) (See RESISTOR REMOVAL/INSTALLATION.)

19. Install the blower motor. (L.H.D.) (See BLOWER MOTOR REMOVAL/INSTALLATION.)

20. Install the car navigation unit. (R.H.D.) (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)

21. Install the glove compartment. (R.H.D.)

22. Install the dashboard. (L.H.D.) (See DASHBOARD REMOVAL/INSTALLATION.)

23. Connect the negative battery cable.