#
ENGINE COOLANT TEMPERATURE (ECT) SENSOR REMOVAL/INSTALLATION [L3 Turbo]

id0140b6801900

  Warning

  • A hot engine can cause severe burns. Turn off the engine and wait until it is cool before removing the ECT sensor.

1. Remove the charge air cooler cover.

2. Drain the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS [L8, LF, L3, L3 Turbo].)

3. Disconnect the ECT sensor connector.

4. Remove the ECT sensor.

5. Install in the reverse order of removal.

Tightening torque

  10-14 N·m
  {1.02-1.42 kgf·m, 7.38-10.32 ft·lbf}

6. Refill the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS [L8, LF, L3, L3 Turbo].)