#
NO. 2 THE DRIVER'S SIDE POWER WINDOW IS INOPERATIVE

id0903j5831100

2 | The driver's side power window is inoperative.
POSSIBLE CAUSE | • Power supply circuit or ground circuit malfunction - Burnt fuse (B+) - Open or short circuit in wiring harness between fuse (B+) and power window main switch - Open or short circuit in wiring harness between power window main switch and power window motor - Open or short circuit in wiring harness between power window main switch and ground • Power window main switch malfunction • Power window motor malfunction • Power window regulator malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Turn the ignition switch to the ON position. • Does the LED on the power window main switch illuminate? | Yes | Go to Step 6.
No | Go to the next step.
2 | • Operate all power windows other than the driver's side window using the power window main switch. • Does the power window operate properly? | Yes | Go to the next step.
No | Inspect for an open or short circuit in the following wiring harnesses. Inspect the connector connections (damage/pulled-out pins, corrosion): • P.WIND 30 A fuse-Power window main switch terminal 1H • Power window main switch terminal 1M-ground. Repair or replace if necessary.
3 | • Is the P.WIND 30 A fuse normal? | Yes | Go to Step 5.
No | Inspect the following: • Short circuit in B+ power supply wiring harness • Short circuit in power window motor Repair or replace if necessary. Replace with the appropriate standard fuse. Then, go to the next step.
4 | • Initialize the power window system. • Operate the power window system. • Do the power windows operate properly? | Yes | Troubleshooting is completed.
No | Re-confirm the symptom and go to Step 1.
5 | • Measure the voltage at the power window main switch terminal 1J. • Is the voltage B+? | Yes | Replace the power window main switch. (See POWER WINDOW SWITCH REMOVAL/INSTALLATION.)
No | Inspect for an open or short circuit in the power window main switch wiring harness (battery power supply). Inspect the power window main switch connector connection. (damage/pulled-out pins, corrosion) Repair or replace if necessary.
6 | • Measure the voltage at the power window main switch. (power window motor output terminal) while operating the power window using the power window main switch. • Is the voltage B+? (Open: terminal 1D/ close: terminal 1B) | Yes | Go to the next step.
No | Replace the power window main switch. (See POWER WINDOW SWITCH REMOVAL/INSTALLATION.)
7 | • Measure the voltage at the power window motor. (battery power supply terminal) while operating the power window using the power window motor. • Is the voltage B+? (Open: terminal F/ close: terminal E) | Yes | Go to the next step.
No | Inspect for an open or short circuit in the wiring harness between the power window main switch and the power window motor. Inspect the power window main switch and power window motor connector connections. (damage/pulled-out pins, corrosion) Repair or replace if necessary.
8 | • Operate the driver's side power window using the power window main switch. • Does the power window motor operate (rotate)? Caution • If the power window motor temperature is high, the motor may not rotate due to the motor internal bimetal function. Leave it untouched for about 3 min to cool it down, then reinspect. | Yes | Go to the next step.
No | Replace the power window motor. (See POWER WINDOW MOTOR REMOVAL/INSTALLATION.)
9 | • Remove the door glass from the carrier plate. • Make sure that the door glass moves smoothly using your hand. • Does the door glass move smoothly? | Yes | Replace the power window regulator. (See POWER WINDOW REGULATOR REMOVAL/INSTALLATION.)
No | Inspect for a bent regulator guide or other possible malfunction. If normal, replace the door glass run-channel.