#
DTC P2122 [L8, LF, L3]

id0102a1811700

DTC P2122 | APP sensor No.1 circuit low input
--- | ---
DETECTION CONDITION | • The PCM monitors the input voltage from APP sensor No.1 when the engine is running. If the input voltage is less than 0.2 V, the PCM determines that the APP sensor No.1 circuit input voltage is low. Diagnostic support note • This is a continuous monitor (CCM). • The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle. • PENDING CODE is available if the PCM detects the above malfunction condition. • FREEZE FRAME DATA is available. • Are any DTCs is stored in the PCM memory.
POSSIBLE CAUSE | • APP sensor No.1 malfunction • Connector or terminal malfunction • Open circuit in wiring harness between APP sensor terminal D and PCM terminal 1AL • Short to ground in wiring harness between APP sensor terminal D and PCM terminal 1AL • Open circuit in wiring harness between APP sensor terminal F and PCM terminal 1AO • Short to ground in wiring harness between APP sensor terminal F and PCM terminal 1AO • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA AND DIAGNOSTIC MONITORING TEST RESULTS HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service information. If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT APP SENSOR CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the APP sensor connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 8.
No | Go to the next step.
4 | INSPECT APP SENSOR NO.1 CIRCUIT FOR SHORT TO GROUND • Turn the ignition switch off. • Inspect for continuity between the following terminals and body ground: - APP sensor terminal D (wiring harness-side) and body ground - APP sensor terminal F (wiring harness-side) and body ground • Is there continuity? | Yes | Repair or replace the wiring harness for a possible short to ground, then go to Step 8.
No | Go to the next step.
5 | INSPECT APP SENSOR NO.1 • Inspect APP sensor No.1. (See ACCELERATOR PEDAL POSITION (APP) SENSOR INSPECTION [L8, LF, L3].) • Is there any malfunction? | Yes | Replace the APP sensor, then go to Step 8. (See ACCELERATOR PEDAL REMOVAL/INSTALLATION [L8, LF, L3].)
No | Go to the next step.
6 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 8.
No | Go to the next step.
7 | INSPECT APP SENSOR NO.1 CIRCUIT FOR OPEN CIRCUIT • Turn the ignition switch off. • Inspect for continuity between the following terminals: - APP sensor terminal D (wiring harness-side) and PCM terminal 1AL (wiring harness-side) - APP sensor terminal F (wiring harness-side) and PCM terminal 1AO (wiring harness-side) • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for a possible an open circuit, then go to the next step.
8 | VERIFY TROUBLESHOOTING OF DTC P2122 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [L8, LF, L3].)
No | Go to the next step.
9 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [L8, LF, L3].) • Is any DTC present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [L8, LF, L3].)
No | DTC troubleshooting completed.