#
DRIVE BELT AUTO TENSIONER INSPECTION [MZR-CD (RF Turbo)]

id0110f1801700

1. Remove the drive belt. (See DRIVE BELT REPLACEMENT [MZR-CD (RF Turbo)].)

2. Verify that the drive belt auto tensioner moves smoothly in the operational direction.

  • Replace the drive belt auto tensioner if necessary.

3. Turn the drive belt auto tensioner pulley by hand and verify that it rotates smoothly.

  • Replace the drive belt auto tensioner if necessary.

4. Install the drive belt.