#
TRANSAXLE OIL INSPECTION [A26MX-R]

id051521800000

1. Park the vehicle on level ground.

2. Remove the oil level plug and washer.

3. Verify that the oil is near the brim of the plug port.

  • If the oil level is low, add the specified amount and type of oil through the filler plug hole.

Manual transaxle oil [A26MX-R]

  Specified oil grade: API Service GL-4 or GL-5
  Specified oil viscosity: SAE 75W-90

4. Tighten the oil level plug with a new washer.

Tightening torque

  27.5-50.9 N·m {2.8-5.1 kgf·m, 37.5-20.2 ft·lbf}