#
SEAT WARMER SWITCH REMOVAL/INSTALLATION

id091300716000

1. Disconnect the negative battery cable.

2. Remove the brake boots panel. (See CONSOLE REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Seat warmer switch (See Seat Warmer Switch Removal Note)
2 | Connector

4. Install in the reverse order of removal.

## Seat Warmer Switch Removal Note

1. Squeeze the tabs of seat warmer switch and pull it forward to remove it.