#
SECONDARY SHAFT COMPONENTS PREINSPECTION

id051500803300

## 1st Gear Thrust Clearance Inspection

1. Measure the 1st gear thrust clearance using a dial indicator.

  • If it exceeds the maximum specification, inspect the contact surfaces of the 1st gear, differential drive gear of the secondary shaft gear, and 1st/2nd clutch hub component. Replace worn and damaged parts.

1st gear thrust clearance

  Standard: 0.05-0.28 mm {0.002-0.011 in}
  Maximum: 0.33 mm {0.013 in}

## 2nd Gear Thrust Clearance Inspection

1. Measure the clearance between 2nd gear and secondary 3rd gear.

  • If it exceeds the maximum specification, inspect the contact surfaces of the 2nd gear, secondary 3rd gear, and 1st/2nd clutch hub component. Replace worn and damaged parts.

2nd gear thrust clearance

  Standard: 0.18-0.46 mm {0.007-0.018 in}
  Maximum: 0.51 mm {0.020 in}