#
PURGE SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF, L3]

id0116a4804300

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Evaporative hose (to charcoal canister) (See Evaporative Hose Installation Note.)
2 | Vacuum hose (to intake manifold) (See Vacuum Hose Installation Note.)
3 | Purge solenoid valve

3. Install in the reverse order of removal.

## Vacuum Hose Installation Note

1. Attach the vacuum hose onto the purge solenoid valve until it contacts the stopper.

## Evaporative Hose Installation Note

1. Attach the evaporative hose onto the purge solenoid valve until it contacts the stopper.