#
CONTROLLER AREA NETWORK (CAN) OUTLINE [L8, LF, L3]

id0140a5104100
• The PCM sends and receives data to and from other modules via the CAN system. Refer to Section 09 for a detailed explanation of the CAN. (See CAN SYSTEM DESCRIPTION.)

## Data sent

• Engine speed
• Vehicle speed
• ATX gear position/selector lever position (ATX)
• Neutral switch position (MTX)
• CPP switch position (MTX)
• Engine torque
• Throttle valve opening angle
• Brake pedal position
• Transaxle specifications
• TCC status (ATX)
• Engine specification
• Immobilizer-related information
• AT warning light on request (ATX)
• Engine coolant temperature
• Travelled distance
• Fuel injection amount
• MIL on request
• Generator warning light on request

## Data received

• Brake system status (EBD/ABS/DSC)
• Wheel speed (LF, RF, LR, RR)
• Fuel tank level
• Immobilizer-related information
• A/C on request
• Transaxle in reverse position