#
STARTER INTERLOCK SWITCH INSPECTION [General (L.H.D.) specs. (MTX)]

id0119a31042a9

  Caution

  • Do not reuse the starter interlock switch if it is removed from the vehicle even once. Replace with a new starter interlock switch when installing.

1. Disconnect the negative battery cable.

2. Disconnect the starter interlock switch connector.

3. Verify that the continuity is as indicated in the table using the tester.

  • If the continuity is not as indicated in the table, replace the starter interlock switch.