#
FRONT COMBINATION LIGHT REMOVAL/INSTALLATION

id091800464400

  Caution

  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the "Discharge headlight service warnings." (See DISCHARGE HEADLIGHT SERVICE WARNINGS.)

  Note

  • When the ignition switch is turned to ON, it is normal to hear the headlight leveling actuator operating for a few second, as it verifies headlight auto leveling system operating condition.

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Connector
2 | Bolt
3 | Clip
4 | Cover
5 | Front combination light

4. Install in the reverse order of removal.

5. Adjust the headlight aiming. (See HEADLIGHT AIMING.)