#
SECONDARY SHAFT (NO.2) COMPONENTS PREINSPECTION

D6E051517040108

## Thrust Clearance Inspection

1. Measure the thrust clearance of each gear using a feeler gauge and a dial gauge.

  Secondary shaft (NO.2) gear thrust clearance
(mm {in})

Gear | Thrust clearance
--- | ---
5th | 0.10-0.55 {0.0039-0.0216}
6th | 0.10-0.55 {0.0039-0.0216}
Reverse | 0.11-0.34 {0.0043-0.0133}

  • If not within the specification, replace the malfunctioning parts.

## Radial Clearance Inspection

1. Measure the radial clearance of each gear using a dial gauge.

  Secondary shaft (NO.2) gear radial clearance
(mm {in})

Gear | Radial clearance
--- | ---
5th | 0.015-0.066 {0.00590-0.00259}
6th | 0.015-0.066 {0.00590-0.00259}
Reverse | 0.015-0.068 {0.00590-0.00267}

  • If not within the specification, replace the malfunctioning parts.