#
LIFTGATE DISASSEMBLY/ASSEMBLY [WGN]

id0911004127a1

1. Disconnect the negative battery cable.

2. Remove the liftgate lower trim. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION [WGN].)

3. To remove the liftgate outer handle and liftgate key cylinder, remove the rear finisher.

4. To remove the stud ball, separate the stud ball and the stay damper.

5. Disassemble in the order indicated in the table.

6. Assemble in the reverse order of disassembly.

1 | Liftgate latch and lock actuator
2 | Liftgate outer handle
3 | Liftgate key cylinder
4 | Clip
5 | Stud ball
6 | Liftgate
7 | Stopper