#
OIL FILTER CONSTRUCTION [L8, LF, L3, L3 Turbo]

id0111b2100800
• The oil filter component is installed on the left surface (vehicle front) of the cylinder block.
• An aluminum oil filter adapter has been adopted for weight reduction. The oil pressure switch and oil cooler are installed on the oil filter adapter.

## Cartridge Type

Oil filter specification

Item | Specification (mm {in})
--- | ---
Outer diameter |  | 65.2-65.8 {2.57-2.59}
Height |  | 72.6-74.4 {2.86-2.92}

• A resin oil filter cover has been adopted for weight reduction. A drain plug has been installed on the bottom of the oil filter cover to improve replacement serviceability.
• An environment-friendly oil filter made of incinerable polyester has been adopted. Only the filter paper needs to be replaced.

.

1 | External view, With oil cooler
2 | Oil cooler
3 | Gasket
4 | Oil pressure switch
5 | Oil filter adapter
6 | Oil filter
7 | Oil filter cover
8 | O-ring
9 | Oil filter drain plug
10 | External view, Without oil cooler
11 | Sectional view
12 | Bypass valve
13 | Oil passage
14 | Normal
15 | Bypass
16 | Spring
17 | Oil pressure

## Spin-on Type

• The oil filter is a full-flow paper element type with an outer diameter of 76.2 mm {3.00 in} and height of 94.0 mm {3.70 in}.

.

1 | External view, With oil cooler
2 | Oil cooler
3 | Gasket
4 | Oil pressure switch
5 | Oil filter adapter
6 | Oil filter
7 | External view, Without oil cooler
8 | Outer diameter
9 | Height