CYLINDER BLOCK INSPECTION

id011000507200

1. Measure the cylinder block for distortion in six directions as shown in the figure using a straight edge and feeler gauge.

  • If it exceeds the maximum specification, replace the cylinder block.

adj2224e089

  Maximum distortion, head gasket side

  0.10 mm {0.004 in}

2. Measure the cylinder bore diameter using the cylinder gauge. The measurement position is in the X and Y directions at a point 42 mm below the top surface of the cylinder as shown in the figure.

  • If not within the specification, replace the cylinder block.

beltze00000021

  Standard cylinder bore diameter

  87.440—87.590 mm {3.4425—3.4484 in}