#
KEYLESS CONTROL MODULE REMOVAL/INSTALLATION [WITH ADVANCED KEYLESS SYSTEM]

id0914z68063b2

  Note

  • If the keyless control module is replaced, always perform the following procedure.

Without immobilizer system

  - Card key programming (See CARD KEY ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM].)
  - Steering lock unit programming (See STEERING LOCK UNIT ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM].)

With immobilizer system

  - Card key programming (See CARD KEY ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM].)
  - Steering lock unit programming (See STEERING LOCK UNIT ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM].)
  - Immobilizer system resetting (with immobilizer system) (See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING [WITH ADVANCED KEYLESS SYSTEM].)

1. Disconnect the negative battery cable.

2. Remove the glove compartment.

3. Remove the bolt.

4. While inclining the keyless control module along the body panel in the direction indicated by the arrow, disengage the bracket tab from the hole in the body panel.

5. Disconnect the keyless control module connector.

6. Remove the keyless control module.

7. Remove the screw, then remove the bracket.

  Note

  • The screw which fixes the keyless control module and bracket is for a body ground connection. Be sure to secure the screw when installing.

8. Install in the reverse order of removal.