#
REAR CROSSMEMBER REMOVAL/INSTALLATION [2WD]

id0214008010a1

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (axle side) and fix it to an appropriate place where the sensor will not be pulled by mistake while servicing the vehicle.

1. Remove the rear auto leveling sensor and harness.

(See REAR AUTO LEVELING SENSOR REMOVAL/INSTALLATION [2WD].) (See REAR AUTO LEVELING SENSOR REMOVAL/INSTALLATION [4WD].)

2. Remove the middle pipe.

(See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF, L3 2WD].)

(See EXHAUST SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

5. Adjust the headlight zeroset.

(See HEADLIGHT ZEROSET.)

6. Inspect the rear wheel alignment.

(See REAR WHEEL ALIGNMENT.)

.

1 | ABS wheel-speed sensor
2 | Parking brake cable
3 | Caliper component (See Caliper Component Removal Note.)
4 | Disc plate
5 | Spindle and hub component (See WHEEL HUB, HUB SPINDLE REMOVAL/INSTALLATION [2WD].)
6 | Bolt (stabilizer control link)
7 | Rear coil spring (See REAR COIL SPRING REMOVAL/INSTALLATION.)
8 | Rear lower arm (See REAR LOWER ARM REMOVAL/INSTALLATION.)
9 | Bolt (rear shock absorber lower side)
10 | Bolt (trailing link front side) (See Bolt (Trailing Link Front Side) Removal Note.) (See Bolt (Trailing Link Front Side) Installation Note.)
11 | Nut (crossmember)
12 | Crossmember component (See Crossmember Component Removal Note.)
13 | Trailing link
14 | Rear lateral link
15 | Rear upper arm
16 | Rear stabilizer
17 | Rear crossmember
18 | Rear crossmember Bushing (See Rear Crossmember Bushing Removal Note.) (See Rear Crossmember Bushing Installation Note.)

## Caliper Component Removal Note

1. Remove the caliper, and suspend it aside with cable.

## Bolt (Trailing Link Front Side) Removal Note

1. Support the trailing link with a jack.

2. Loosen the bolt (lateral link inner side).

## Crossmember Component Removal Note

  Warning

  • Removing the crossmember is dangerous. The crossmember component could fall and cause serious injury or death. Verify that the jack securely supports the crossmember component.

1. Support the crossmember component using a jack and remove the nuts.

2. Remove the crossmember component.

## Rear Crossmember Bushing Removal Note

1. Remove the bushing using screw driver (-), being care not to damage the rear crossmember.

## Rear Crossmember Bushing Installation Note

1. Set the bushings as shown in the figure.

2. Tap the bushing onto the rear crossmember using the SSTs.

## Bolt (Trailing Link Front Side) Installation Note

1. Support the trailing link with a jack.

2. Tighten the bolts (trailing link front side).