#
MANUAL MODE SHIFT CONTROL OPERATION [JA5AX-EL]

id051705102800

## Manual Mode Shift

• When the selector lever is shifted over from the D to M range position, the M range switch in the selector lever component turns on, sending a manual mode command signal to the PCM which activates the manual mode shift control.
• When in manual mode and the selector lever is operated in the back (+) direction, the up switch in the selector lever component is turned on and an up-shift command signal is inputted to the PCM.

  - The PCM, triggered by the up-shift command signal, carries out shifting by outputting an operation signal to the shift solenoid if the ATF temperature is not low (for 3GR only), vehicle speed is higher than the set speed and the gear position is 3GR or lower.

• Conversely, when the selector lever is operated in the forward (-) direction, the down switch in the selector lever component turns on, and a down-shift command signal is inputted to the PCM.

  - The PCM, triggered by the down-shift command signal, carries out shifting by outputting an operation signal to the shift solenoid if the vehicle speed is less than the set speed and the gear position is 2GR or above.

• The PCM utilizes a specialized M range automatic shift diagram when down shifting. This restriction of manual downshifting is carried out to reduce load on the ATX and prevent engine over-revving.

Condition | Shift control | Note
--- | --- | ---
2GR→ 3GR up-shift command at low speed | • To reduce load on the ATX, upshifting is inhibited until vehicle reaches speed possible for upshifting | -
3GR→ 4GR up-shift command at low speed
3GR→ 4GR up-shift command, low ATF temperature | • To reduce load on the ATX, upshifting to 4GR is inhibited
4GR→ 3GR down-shift command, above set speed | • To prevent engine over-rev, downshifting is inhibited until vehicle reaches speed possible for downshifting | • Selector indicator "M" light and gear position indicator light flash to alert driver
3GR→ 2GR down-shift command, above set speed
2GR→ 1GR down-shift command, above set speed
In 4GR deceleration, speed goes below coast-down set speed (deceleration down- shift) | • To assure drive stability, automatically downshifts from 4GR to 3GR | -
In 3GR deceleration, speed goes below coast-down set speed (deceleration down- shift) | • To assure drive stability, automatically downshifts from 3GR to 1GR
In 2GR deceleration, speed goes below coast-down set speed (deceleration down- shift) | • To assure driving stability, automatically downshifts from 2GR to 1GR

Shift diagram

.

1 | TCC operation available
2 | Throttle opening
3 | TCC operation OFF
4 | TCC operation ON
5 | Vehicle speed (km/h {mph})
6 | Down shifting is inhibited until vehicle reaches speed possible for downshifting
7 | When decelerating below set vehicle speed, executes automatic downshifting