#
PLASTIC PARTS HEAT RESISTING TEMPERATURE

D6E098050000B01

Part Name | Code | Material Name | Heat resisting TemperatureC°{F°}
--- | --- | --- | ---
WINDSHIELD MOULDING | PVC | POLYVINYLCHLORIDE | 95 {203}
COWL GRILLE | PP | POLYPROPYLENE | 95 {203}
FRONT COMBINATION LIGHT | LENS | PC | POLYCARBONATE | 130 {266}
HOUSING | PBT | PBT | 120 {248}
RADIATOR GRILLE | GRILLE | ABS | ABS | 90 {194}
REINFORCE-MENT | PP | POLYPROPYLENE | 95 {203}
FRONT BUMPER | PP | POLYPROPYLENE | 100 {212}
FRONT SIDE MARKER LIGHT | LENS | PMMA | ACRYLIC | 75 {167}
HOUSING | AAS | AAS | 120 {248}
OUTER MIRROR | HOUSING | ABS | ABS | 95 {200}
BASE | PBT | PBT | 200 {395}
BLACK | AES | AES | 75 {167}
BODY COLOR | ABS | ABS | 90 {194}
MIRROR HOLDER | PP | POLYPROPYLENE | 50 {122}
REAR COMBINATION LIGHT | LENS | PMMA | ACRYLIC | 80 {167}
HOUSING | AAS | AAS | 70 {158}
OUTER HANDLE | HANDLE BASE | PC-PET | POLYCARBONATE-PET | 80 {167}
HANDLE LEVER | PC-PBT | POLYCARBONATE-PBT | 80 {167}
REAR BUMPER | PP | POLYPROPYLENE | 100 {212}
REAR FINISHER | ABS | ABS | 90 {194}
HIGH-MOUNT BRAKE LIGHT (5HB) | PC | POLYCARBONATE | 130 {266}
ROOF MOULDING | PVC | POLYVINYLCHLORIDE | 95 {203}
BELTLINE MOLDING | PVC | POLYVINYLCHLORIDE | 95 {203}
REAR SPOILER | ABS | ABS | 90 {194}
SIDE STEP MOLDING | PP | POLYPROPYLENE | 100 {212}
ROOF RAIL | PP | POLYPROPYLENE | 100 {212}
SHROUD PANEL | PP | POLYPROPYLENE | 100 {212}

  Note

  • The application of temperatures higher then heat resisting temperatures may result in part deformation.