#
STEERING LOCK UNIT ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM]

id0914z68073b2

  Caution

  • Do not place the following devices in the vehicle while programming, otherwise programming cannot be performed.

  - WDS or equivalent
  - Personal computer
  - Device that can send/receive radio waves

  Note

  • The steering lock unit and steering lock component are a single unit. Therefore, replace the steering lock component when replacing steering lock unit. (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)
  • For this procedure, a programmed card key is necessary. If there is no programmed card key, perform the steering lock unit programming after the card key programming.

1. Bring the programmed card key into the vehicle.

2. Fully lower the driver-side door glass.

3. Connect the WDS or equivalent to the DLC-2.

4. Pull out the WDS or equivalent cable from the door glass opening and set the WDS or equivalent outside the vehicle.

5. Select "BODY/SECURITY/PATS (immobilizer)" from the WDS or equivalent screen menu.

6. Perform the security access according to the directions on the WDS or equivalent screen. (See SECURITY ACCESS PROCEDURE.)

7. The security access begins and the WDS or equivalent displays "OUT-CODE".

  Note

  • When "OUT-CODE" is first displayed, turning the ignition switch from the LOCK to the ON position 5 times will change the "OUT-CODE".

8. Input the "IN-CODE" that corresponds to the "OUT-CODE" displayed on the WDS or equivalent screen.

9. Select "STEERING LOCK UNIT PROGRAMMING" and perform procedures according to the directions on the WDS or equivalent screen.