#
NEUTRAL SWITCH CONSTRUCTION/OPERATION [MZR-CD (RF Turbo)]

id0140f1176900
• While the shift lever is in the neutral position, the contact point closes (ON) and the PCM detects below 1.0 V. While the shift lever is not in the neutral position, the contact point opens (OFF) and the PCM detects B+.

.

1 | Neutral switch
2 | Push on
3 | Neutral (switch ON)
4 | Not in neutral (switch OFF)
5 | No load
6 | Loaded