#
THEFT-DETERRENT SYSTEM OUTLINE

id0914b5100500
• The theft-deterrent system includes sound and light alarms that activate when the bonnet, the trunk lid (4SD) or liftgate (5HB, WGN), or a door is opened by means other than the transmitter. The turn lights flash and the horn and the theft-deterrent siren sound.
• When the transmitter unlock button is pressed, the alarms stop.
• An intruder sensor has been installed in the forward part of the roof (4SD, 5HB: without sliding sunroof, WGN: with sliding sunroof) or in the center part of the roof (4SD, 5HB: with sliding sunroof, WGN: without sliding sunroof). The intruder sensor senses movement in the vehicle based on radio waves, and sends an alert signal to the theft-deterrent control module.
• An intruder sensor has been installed in the rear part of the roof. (WGN)
• A theft-deterrent siren has been installed on the rear, left side of the trunk (4SD) or liftgate (5HB, WGN). The theft-deterrent siren includes an internal back-up power supply so that if power from the battery is cut by any means, the siren will still sound.