#
OIL COOLER CONSTRUCTION [MZR-CD (RF Turbo)]

id0111f1100900
• A water-cooled type oil cooler has been adopted to reduce engine oil degradation.
• There are two types of oil coolers, a 5-layered (High power) and a 4-layered (Standard power) type, based on the difference in engine output.
• The oil cooler is installed on the right surface (vehicle rear) of the cylinder block.

.

1 | External view
2 | Sec. A-A, 5-layered type
3 | Engine coolant flow direction