#
CURTAIN AIR BAG MODULE REMOVAL/INSTALLATION

id081000800900

  Warning

  • Handling the air bag module improperly can accidentally deploy the air bag module, which may seriously injure you. Read the service warnings and cautions before handling the air bag module. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.)

1. Turn the ignition switch to the LOCK position.

2. Disconnect the negative battery cable and wait for 1 min or more.

3. Remove the headliner. (See HEADLINER REMOVAL/INSTALLATION [4SD, 5HB].) (See HEADLINER REMOVAL/INSTALLATION [WGN].)

4. Remove in the order indicated in the table.

1 | Connector
2 | Bolt
3 | Curtain air bag module

5. Install in the reverse order of removal.

6. When the ignition switch is turned to the ON position verify that the air bag system warning light illuminates for approx. 6 s and goes out.

  • If the air bag system warning light does not operate normally, refer to the on-board diagnostic system (air bag system) and perform inspection of the system.

## Connector Removal Note

1. Using a flathead screwdriver, pry out the connector's stopper plate.

2. Disconnect the connector.

## Curtain Air Bag Module Installation Note (4SD Right Side)

1. Pass the curtain air bag module harness through the hole in the body.