#
DTC P0607 [MZR-CD (RF Turbo)]

id0102f1809500

DTC P0607 | PCM performance problem
--- | ---
DETECTION CONDITION | • PCM internal malfunction. Diagnostic support note • MIL does not comes on. • PENDING CODE is available if PCM detects the above malfunction condition. • FREEZE FRAME DATA is not available. • DTC is stored in PCM memory.
POSSIBLE CAUSE | • PCM internal malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record FREEZE FRAME DATA on repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Check for related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to available repair information. • If vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY TROUBLESHOOTING OF P0607 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear DTC from PCM memory using the WDS or equivalent. • Start the engine. • Is same DTC present? | Yes | Replace the PCM, go to the next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
4 | VERIFY AFTER REPAIR PROCEDURE • Perform "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].) • Is any DTC present? | Yes | Go to applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Troubleshooting completed.