#
GENERATOR CONSTRUCTION [L3 Turbo]

id0117b11023b2
• With the elimination of the voltage regulator, generator control is carried out by the PCM. Excitation current in the field coil is increased or decreased by the duty signal from the PCM sent to the power transistor built into the generator.
• Two delta connection type stator coils have been adopted.
• A generator duct and a generator heat insulator made of plastic have been adopted to protect the generator from the exhaust manifold heat.

.

1 | Pulley
2 | Front cover
3 | Front bearing
4 | Rotor
5 | Rear bearing
6 | Stator coil
7 | Regulator component (built-in power transistor)
8 | Rectifier
9 | Rear cover
10 | Terminal B component
11 | Heat insulator

.

1 | Stator coil
2 | Power transistor
3 | Instrument cluster (warning light)
4 | Battery
5 | Dummy

• The phase difference in the circuit of the two stator coils causes the electromagnetic pull between the rotor and the stator to be eliminated logically. Due to this, electromagnetic vibration and generator operation noise (electromagnetic noise) have been reduced.

1 | Phase difference
2 | Stator coil

• The pulsation occurring through voltage rectifying is minimized, as a result, stable voltage output is supplied due to the adoption of two stator coils with the phase difference.

.

1 | Voltage (V)
2 | Angle (°)
3 | Stator coil (includes 1 type)
4 | Stator coil (includes 2 type)
5 | Rectified voltage

• The generator warning light in the instrument cluster illuminates under the following conditions.

  - Charging system voltage problem
  - Charging system voltage low input
  - Charging system voltage high input
  - IAT sensor circuit low input
  - IAT sensor circuit high input