#
POWER WINDOW MOTOR INSPECTION

id091200417000

## Driver's Side

1. Disconnect the power window motor connector.

2. Apply battery positive voltage to the power window motor terminals E and F and inspect the operation the power window motor operation.

  • If there is any malfunction, replace the power window motor.

Motor operation | Terminal
--- | ---
F | E
UP | GND | B+
DOWN | B+ | GND

3. Apply battery positive voltage to the power window motor terminal D and connect terminal C to ground.

4. Measure the voltage at terminal B and A while performing Step 3.

  • If there is any malfunction, replace the power window motor.

Voltage

  Pulse wave: MAX. 5 V, MIN. 0 V

## Except Driver's Side

1. Apply battery positive voltage to the power window motor terminals and inspect the operation of the power window motor.

  • If there is any malfunction, replace the power window motor.

Motor operation | Terminal
--- | ---
F | E
UP | GND | B+
DOWN | B+ | GND