#
GLOW PLUG REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

id0113f1804400

  Caution

  • Do not damage the heated section of the glow plug.
  • Do not reuse a glow plug that has been dropped over a height of 10 cm {0.4 in}, even when there are no scratches and resistance is normal (approx. 0.6 ohms [20°C {68°F}] (Reference value)).
  • Do not remove the glow plug unless you are replacing it.

1. Disconnect the negative battery cable.

2. Remove the engine cover.

3. Remove in the order indicated in the table.

1 | Glow plug lead
2 | Glow plug (See Glow Plug Removal Note) (See Glow Plug Installation Note)

4. Install in the reverse order of removal.

## Glow Plug Removal Note

1. When removing the glow plug, first loosen it at least one pitch using a tool, then loosen by hand.

## Glow Plug Installation Note

1. Tighten the glow plug at least one pitch by hand, and continue tightening with a tool.