#
FUEL TANK INSPECTION [L3 Turbo]

id0114b4803200

  Caution

  • Disconnecting/connecting the quick release connector without cleaning it may cause damage to the fuel pipe and quick release connector. Always clean the quick release connector joint area before disconnecting/connecting using a cloth or soft brush, and make sure that it is free of foreign material.

  Note

  • This inspection is for two rollover valves integrated in the fuel tank.

1. Disconnect the plastic fuel hose and the fuel pump unit connector. (See FUEL PUMP UNIT REMOVAL/INSTALLATION [L3 Turbo].)

2. Remove the fuel tank with the fuel pump unit. (See FUEL TANK REMOVAL/INSTALLATION [L3 Turbo].)

3. Plug the port as shown in the figure.

4. Level the fuel tank.

5. Blow through port B and verify that there is airflow from port A.

  • If there is no airflow, replace the fuel tank.
  • If there is airflow, turn the fuel tank upside down, and proceed to Step 6.

6. Blow through port B and verify that there is no airflow from port A.

  • If there is airflow, replace the fuel tank.