#
EVAPORATIVE GAS CHECK VALVE (ONE-WAY) INSPECTION (L.H.D.) [L8, LF, L3]

id0116a48194a8

1. Remove the evaporative gas check valve (one-way).

2. Apply pressure to port A, and verify that there is no airflow.

  • If there is airflow, replace the evaporative gas check valve (one-way).

3. Apply negative pressure to port A, and verify that there is air flow.

  • If there is no airflow, replace the evaporative gas check valve (one-way).