#
FUEL WARMER FUNCTION (COLD DISTRICT SPECIFICATIONS) [MZR-CD (RF Turbo)]

id0114f11482d0
• If fuel for the summer season is used in the winter season, the wax component in the fuel may become greasy when the temperature is cold. After the engine is started, the fuel warmer melts the greasy wax component to prevent a clogging in the fuel filter.

1 | Priming pump
2 | Fuel warmer (Cold district specification)
3 | Fuel filter
4 | Drain plug