#
ENGINE OIL LEVEL INSPECTION [L3 Turbo]

id0111b28005b4

1. Position the vehicle on level ground.

2. Warm up the engine to normal operating temperature.

3. Stop the engine and wait for 5 min.

4. Remove the dipstick and verify that the oil level is between the MIN and MAX marks on the dipstick and inspect the engine oil condition.

  • If the oil level is below the MIN mark, add the recommended engine oil.
  • If necessary, replace with the recommended engine oil.