#
REAR STABILIZER REMOVAL/INSTALLATION [4WD]

id0214008005a2

1. Remove the rear auto leveling sensor.

(See REAR AUTO LEVELING SENSOR REMOVAL/INSTALLATION [2WD].) (See REAR AUTO LEVELING SENSOR REMOVAL/INSTALLATION [4WD].)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

4. Adjust the headlight zeroset.

.

1 | Stabilizer control link
2 | Coil spring component (One side only)
3 | Stabilizer bracket
4 | Bushing
5 | Bolt (Differential front side) (See Bolt (Differential Front Side) Removal Note.) (See Bolt (Differential Front Side) Installation Note.)
6 | Rear stabilizer

## Bolt (Differential Front Side) Removal Note

1. Disconnect differential oil temperature sensor connector and 4WD solenoid connector.

2. Support the differential with a jack as shown in the figure.

3. Remove the bolt.

## Bolt (Differential Front Side) Installation Note

1. Support the differential with a jack, and then install the bolt.

2. Connect differential oil temperature sensor connector and 4WD solenoid connector.