#
MULTIPLE FUEL INJECTION CONTROL OUTLINE [MZR-CD (RF Turbo)]

id0140f1738300
• Pilot injection: To reduce noise and NOx, the PCM performs multiple fuel injections before the main injection according to the vehicle driving conditions. Follow-up injection, post injection: To increase exhaust gas temperature for diesel particulate filter regeneration, the PCM performs fuel injection after the main injection.