DRIVE BELT AUTO TENSIONER INSPECTION [L3 Turbo]

id0110b3801700

1. Remove the drive belt. (See DRIVE BELT REPLACEMENT [L3 Turbo].)

2. Verify that the drive belt auto tensioner moves smoothly in the operational direction.

  • Replace the drive belt auto tensioner if necessary.

  Drive belt auto tensioner tightening torque

  19—25 N·m {2.0—2.5 kgf·m, 15—18 ft·lbf}

e6u110zwb036

3. Rotate the drive belt auto tensioner pulley by hand and verify that it rotates smoothly.

  • Replace the drive belt auto tensioner if necessary.

  Drive belt auto tensioner tightening torque

  19—25 N·m {2.0—2.5 kgf·m, 15—18 ft·lbf}

4. Install the drive belt. (See DRIVE BELT REPLACEMENT [L3 Turbo].)