#
REMOTE CONTROL AND CRADLE CONSTRUCTION/OPERATION

id092000106300
• The remote control and cradle are located on the console.
• The buttons and joystick for controlling car-navigation are located on the top side of the remote control. The infrared transmitter sends signals through a terminal on the front and back of the remote control.
• An infrared sensor that receives signals from the remote control is located on the cradle. The received signals are sent to the LCD unit.
• The remote control uses the batteries as a power source when not in the cradle and uses the power supply connector when set in the cradle. (Ignition switch at ACC or ON position)

  Note

  • The batteries are not charged when the remote control is in the cradle.

.

1 | Remote control
2 | Cradle
3 | Front view
4 | Top view
5 | Underside view
6 | Infrared transmitter
7 | Infrared sensor
8 | Power supply connector

No. | Button (component) | Function
--- | --- | ---
9 | [POS (Position)] button | Displays the current position.
10 | Joystick | Selects items by tilting it up, down, right and left.
11 | [ENTER] button | Executes a selected item.
12 | [ZOOM] button | Changes the map scale.
13 | [RET] button | Returns to the previous screen.
14 | [MENU] button | Select a menu.
15 | [VOICE] button | Initiates vocal guidance for route maneuvers.