#
NO.22 VIBRATION CONCERNS (ENGINE) [L8, LF, L3]

id0103a1802800

22 | VIBRATION CONCERNS (ENGINE)
--- | ---
DESCRIPTION | • Vibration from under hood or driveline
POSSIBLE CAUSE | • Loose attaching bolts or worn parts • Components malfunction such as worn parts

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Inspect the following components for loose attaching bolts or worn parts: • Cooling fan • Drive belt and pulleys • Generator • Engine mounts • Exhaust system mounts All items normal? | Yes | Inspect the following systems: • Wheels • ATX • Driveline • Suspension
No | Readjust or retighten engine mount installation position. Service if necessary for other parts.
2 | • Verify test results. - If normal, return to diagnostic index to service any additional symptoms. (See ENGINE SYMPTOM TROUBLESHOOTING [L8, LF, L3].) - If malfunction remains, inspect related Service Information and perform repair or diagnosis. • If vehicle is repaired, troubleshooting completed. • If vehicle is not repaired or additional diagnostic information is not available, replace the PCM. (See PCM REMOVAL/INSTALLATION [L8, LF, L3].)