#
KEYLESS BUZZER REMOVAL/INSTALLATION

id0914z6810600

1. Disconnect the negative battery cable.

2. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

3. Remove the front door speaker. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove the screws.

5. Disconnect the connector.

6. Remove the keyless buzzer from the speaker installation hole.

7. Install in the reverse order of removal.