#
ACTIVE COMMAND MODE TABLE [HEADLIGHT AUTO LEVELING SYSTEM]

id0902i7466000

## LHID

Command name | Definition
--- | ---
CALAXLSN# | Command for headlight zeroset use (See HEADLIGHT ZEROSET)

  Note

  • Select the following four commands at the same time and carry out simulation inspection.

Command name | Definition | Operation | Note
--- | --- | --- | ---
HDL_POS# | Select "Calibration" operation, verify that the headlight actuator moves to the position at time of headlight zeroset | Calibration/High/Low/Auto | Ignition key at ON (Engine OFF), and headlight ON
Select "High" operation, verify that headlight actuator moves upward
Select "Low" operation, verify that headlight actuator moves downward
Select "Auto" operation, verify that headlight actuator is under automatic control