#
TRANSAXLE RANGE (TR) SWITCH CONSTRUCTION/OPERATION [FS5A-EL]

id051721109200
• A variable resistor type switch has been adopted for the transaxle range switch.
• Because the transaxle range switch and the selector lever are connected by the selector cable, the transaxle range switch indicates a specified resistance according to selector lever operation and from this the TCM determines the selector lever position. The corresponding signal are sent from the TCM to other related parts.

.

1 | TR switch
2 | Instrument cluster
3 | M range switch
4 | Up switch
5 | Down switch