#
FRONT DOOR TRIM REMOVAL/INSTALLATION

id091700459700

## Driver's Side

1. Disconnect the negative battery cable.

2. Remove the inner garnish.

3. Open the cap using a small screwdriver, then remove the screw.

4. Remove the inner handle cover.

5. Remove the inner garnish.

6. Remove the cover, then remove screw A.

7. Remove the lens cover, then remove screw.

8. Disengage clips A from the front door using a fastener remover.

9. Pull the front door trim upward, then disengage tabs B from the front door.

10. Disconnect the power door mirror switch connector and the power window main switch connector.

11. Remove the courtesy light.

12. Remove the front door trim.

13. Remove the switch panel from the front door trim.

14. Install in the reverse order of removal.

## Passenger's Side

1. Disconnect the negative battery cable.

2. Remove the inner garnish.

3. Open the cap using a small screwdriver, then remove the screw.

4. Remove the inner handle cover.

5. Remove the cover, then remove screw A.

6. Remove the lens cover, then remove screw.

7. Disengage clips A from the front door using a fastener remover.

8. Pull the front door trim upward, then disengage tabs B from the front door.

9. Disconnect the power window subswitch connector.

10. Remove the courtesy light.

11. Remove the front door trim.

12. Remove the switch panel from the front door trim.

13. Install in the reverse order of removal.