#
SPARK PLUG CONSTRUCTION [L8, LF, L3, L3 Turbo]

id0118a4100400
• An iridium spark plug with excellent durability and firing performance has been adopted.
• The extremely thin, center electrode has a diameter of 0.6 mm {0.024 in} and is made of iridium alloy.
• Durability has been improved by the use of a platinum-tipped grounding electrode.
• Based on the thinner electrode (center electrode), electric discharge has been reduced and ignition has been improved, resulting in stable ignition performance under all driving conditions.

1 | Iridium alloy
2 | Platinum-tip
3 | Center electrode