#
FRONT SIDE MARKER LIGHT REMOVAL/INSTALLATION

id091800810400

1. Disconnect the negative battery cable.

2. Partially peel off the mudguard.

3. Remove in the order indicated in the table.

1 | Front side marker light (See Front Side Marker Light Removal Note)
2 | Connector
3 | Socket
4 | Front side marker light bulb

4. Install in the reverse order of removal.

## Front Side Marker Light Removal Note

1. Insert your hand into where the mud guard is bent back and push the tab to remove the front side marker light.

2. Pull the front side marker light toward you to remove it.