#
CARD KEY (TRANSMITTER) CONSTRUCTION/OPERATION

id0914b5103200
• A card-type transmitter that is thin and convenient to carry has been adopted.
• A maximum of six transmitters can be programmed for one vehicle.
• A built-in operation indicator light illuminates according to LOCK/UNLOCK button operation and request signal from the vehicle.
• In case the transmitter is inoperable due to battery depletion, the doors can be locked/unlocked and the engine can be started using the auxiliary key.
• A transponder is built into the auxiliary key for vehicles with the immobilizer system.

1 | Indicator light
2 | Lock button
3 | Unlock button
4 | Intruder sensor cut-off button (with theft-deterrent system)
5 | Auxiliary key
6 | Transmitter