TIMING BELT DISASSEMBLY [WITH DIESEL PARTICULATE FILTER]

id0110f3500300

1. Disassemble in the order indicated in the table.

dpe110ze1050

1 | Pulley cover
2 | Crankshaft pulley (SeeCrankshaft Pulley Disassembly Note)
3 | Timing belt cover
4 | Timing belt, timing belt auto tensioned (SeeTiming Belt, Timing Belt Auto Tensioner Disassembly Note)
5 | Idler
6 | Supply pump pulley (SeeSupply Pump Pulley Disassembly Note)
7 | Timing belt pulley (SeeTiming Belt Pulley Disassembly Note)
8 | Gear cover
9 | Drive gear (SeeDrive Gear Disassembly Note)
10 | Camshaft position sensor
11 | Gear case
12 | Camshaft pulley (SeeCamshaft Pulley Disassembly Note)
13 | Tensioner
14 | Seal plate

Crankshaft Pulley Disassembly Note

1. Hold the crankshaft using the SST.

2. Remove the crankshaft pulley lock bolt.

bej0110e003

Timing Belt, Timing Belt Auto Tensioner Disassembly Note

1. Turn the crankshaft clockwise and align the timing marks as shown.

dpe110bw1010

  Caution
  • The following will damage the belt and shorten its life; forcefully twisting it, turning it inside out, or allowing oil or grease on it.
  • After removing the timing belt, do not move the crankshaft or the camshaft pulley or both from this position because it can cause the valve and piston to contact.

2. Remove the timing belt auto tensioner.

3. Mark the timing belt rotation on the belt for proper reinstallation.

dpe110ze1004

Supply Pump Pulley Disassembly Note

1. Verify that timing marks are correctly aligned.

  Caution
  • Do not fully tighten the anti-rotation bolt to prevent damage to the supply pump bracket and supply pump pulley.

2. Hold the supply pump pulley using the SST and remove the supply pump pulley lock nut.

am6zzw00003642

3. Separate the supply pump pulley from the supply pump shaft using the SST.

am6zzw00003643

Timing Belt Pulley Disassembly Note

1. Hold the crankshaft using the SST.

2. Remove the timing belt pulley lock bolt.

bej0110e003

3. Remove the timing belt pulley using the SST.

bej0110e008

Drive Gear Disassembly Note

1. Hold the camshaft using the SST.

2. Remove the drive gear lock bolt.

dpe110ze1038

Camshaft Pulley Disassembly Note

1. Hold the camshaft using the SST.

2. Remove the camshaft pulley lock bolt.

bej0110e009

3. Remove the camshaft pulley using the SST.

bej0110e010