#
AUTOMATIC TRANSAXLE CONTROL SYSTEM WIRING DIAGRAM [JA5AX-EL]

id051705102000

.

1 | TCM
2 | R position (TR switch)
3 | D range (TR switch)
4 | N position (TR switch)
5 | P position (TR switch)
6 | Brake switch
7 | M range switch
8 | Up switch
9 | Down switch
10 | Selector lever
11 | TFT sensor
12 | VSS
13 | Input/turbine speed sensor
14 | Intermediate sensor
15 | Pressure control solenoid
16 | 2-4 brake solenoid valve
17 | High clutch solenoid valve
18 | TCC solenoid valve
19 | Shift solenoid A
20 | Shift solenoid B
21 | Shift solenoid C
22 | Reduction timing solenoid valve
23 | Neutral shift solenoid valve
24 | CAN_L
25 | CAN_H
26 | Instrument cluster
27 | PCM
28 | ABS HU/CM or DSC HU/CM