#
CLUTCH HOUSING AND TRANSAXLE CASE COMPONENTS ASSEMBLY

D6E051517011102

## Assembly Components

1 | Clutch housing
2 | Differential component
3 | Primary shaft component
4 | Secondary shaft (No.1) component
5 | Secondary shaft (No.2) component
6 | Needle bearing
7 | Reverse idler gear
8 | Thrust washer
9 | Reverse idler gear shaft
10 | 1st/2nd shift fork
11 | Counter lever
12 | 3rd/4th control rod end (A)
13 | 3rd/4th control rod (A)
14 | Counter lever pivot
15 | Snap ring
16 | 3rd/4th shift fork
17 | 1st/2nd control rod
18 | 3rd/4th control rod end (B)
19 | 3rd/4th control rod (B)
20 | Spring pin
21 | Shift fork retaining bolt
22 | Spring pin
23 | Spring pin
24 | Reverse shift fork
25 | 5th/6th shift fork
26 | Reverse control rod
27 | 5th/6th control rod
28 | Shift fork retaining bolt
29 | Shift fork retaining bolt
30 | Baffle plate
31 | Sealing cap, spring seat, detent spring, detent ball
32 | Transaxle case
33 | Sealing cap
34 | Reverse idler shaft retaining bolt
35 | Shift component
36 | Select lever set

1 | Clutch housing
2 | Magnet
3 | Primary shaft oil seal
4 | Primary shaft front bearing
5 | Oil funnel
6 | Secondary shaft (No.1) front bearing
7 | Bearing cover
8 | Bearing cover
9 | Oil funnel
10 | Secondary shaft (No.2) front bearing outer race
11 | Differential side bearing outer race
12 | Differential oil seal
13 | Pivot pin
14 | Transaxle case
15 | Snap ring
16 | Snap ring
17 | Oil pass
18 | Adjust shim
19 | Secondary shaft (No.2) rear bearing outer race
20 | Adjust shim
21 | Differential side bearing outer race
22 | Control rod bearing
23 | Shift lever shaft bearing
24 | Differential oil seal
25 | Sealing cap
26 | Neutral switch
27 | Select push pin
28 | Back-up light switch
29 | Shift push pin
30 | Straight pin
31 | Oil level plug
32 | Drain plug
33 | Knock ring

## Assembly Procedure

1. Install a new primary shaft oil seal in the clutch housing using the SST.

  Oil seal press-in depth
  4.4-5.0 mm {0.17-0.19 in}

2. Install a new primary shaft front bearing using the SST.

3. Install the oil funnel for in the secondary shaft (No.1 and No.2) to the clutch housing.

  Note

  • Align the clutch housing groove and the funnel projection, and insert.
  • Lubrication hole can be positioned either on the left or right.

4. Install a new secondary shaft (No.1) front bearing using the SST.

5. Install the secondary shaft (No.2) front bearing outer race using the SST.

6. Install the primary shaft bearing cover and secondary shaft (No.1) bearing cover.

  Tightening torque
  6.8-15.8 N·m
  {69.4-161 kgf·cm, 60.2-139 in·lbf}

7. Install the differential side bearing outer race to the clutch housing using the SST.

(Except L3 Turbo)

(L3 Turbo)

8. Install the differential side bearing outer race and adjust shim to the transaxle case using the SST.

  Note

  • Use the adjust shim selected in the differential side bearing preload adjustment.
  (See DIFFERENTIAL SIDE BEARING PRELOAD ADJUSTMENT.)

9. Install a new differential oil seal to the clutch housing using the SST.

(4x2)

(4x4)

10. Install the secondary shaft (No. 2) rear bearing outer race and adjust shim to the transaxle case using the SST.

  Note

  • Use the adjust shim selected in the secondary shaft (No. 2) bearing preload adjustment.
  (See SECONDARY SHAFT (NO.2) BEARING PRELOAD ADJUSTMENT.)

11. Install a new differential oil seal to the transaxle case using the SST.

  Oil seal press-in depth
  -0.5-0.5 mm {-0.019-0.019 in}

12. Install the new control rod bearings to the clutch housing and transaxle case using the SST.

  Note

  • Assembling direction can be either way.

  Bearing press-in depth
  0-0.5 mm {0-0.019 in}

13. Install a new shift lever shaft bearing to the transaxle case using the SST.

  Note

  • Assembling direction can be either way.

  Bearing press-in depth
  0-0.5 mm {0-0.019 in}

14. Install the snap rings to the transaxle case.

15. Install each gear component.

  (1) Install the differential to the clutch housing.

  Caution

  • Installing the primary shaft can damage the oil seal, reducing the performance of the transaxle. When installing the primary shaft to the clutch housing, be careful not to damage it.

  (2) Install the primary shaft component and secondary shaft (No.1) component to the clutch housing at the same time.
  (3) Install the secondary shaft (No.2) component.
  (4) Install the reverse idler gear, needle bearing, thrust washer, and reverse idler gear shaft.

  Caution

  • Align the thrust washer rotation lock projection and reverse idle gear shaft groove.
  • Position the shaft direction as shown in the figure for the transaxle case assembly.

16. Install the 1st/2nd shift fork.

17. Install the counter lever and 3rd/4th control rod (A).

18. Install the counter lever pivot and secure it with the snap ring.

19. Install the 3rd/4th shift fork and then install the 1st/2nd control rod ball groove in the direction shown in the figure.

20. Install 3rd/4th control rod end (B) so that it engages with the counter lever as shown in the figure.

21. Install the 3rd/4th control rod (B) ball groove in the direction shown in the figure.

22. Tap in 3rd/4th control rod end (A and B) new spring pins shown in the figure.

23. Tap in 3rd/4th shift fork spring pin using a pin punch.

24. Install the 1st/2nd shift fork retaining bolt.

  Tightening torque
  15.7-23.5 N·m
  {1.7-2.3 kgf·m, 11.6-17.3 ft·lbf}

25. Install the 5th/6th shift fork and reverse shift fork.

26. Install the 5th/6th control rod and reverse control rod being careful of the ball groove direction.

27. Install the reverse shift fork retaining bolt and 5th/6th shift fork retaining bolt.

  Tightening torque
  15.7-23.5 N·m
  {1.7-2.3 kgf·m, 11.6-17.3 ft·lbf}

28. Install the baffle plate.

  Tightening torque
  6.0-11.0 N·m
  {61.2-112.1 kgf·cm, 53.2-97.3 in·lbf}

29. Install the detent ball, detent spring, detent spring seat, and sealing cap to the clutch housing.

30. Install the magnet to the clutch housing.

31. Install the oil pass to the transaxle case.

32. Install the transaxle case.

  (1) Apply a light coat of silicone sealant to the contact surfaces of the transaxle case and the clutch housing.
  (2) Place the transaxle case on the clutch housing.
  (3) Install the bolt (M8 x 1.25) to the secondary shaft (No. 1) through the sealing cap hole.
  (4) While pulling up the secondary shaft (No. 1) installation bolt, widen the snap ring, and then fix the snap ring into the secondary shaft bearing groove as shown in the figure.
  (5) While pushing up the primary shaft from the clutch housing side, widen the snap ring (primary shaft side) and fix it into the primary shaft bearing groove.
  (6) Measure the center-to-center distance of the respective snap ring holes as shown in the figure and verify that the snap ring is properly installed in the bearing groove.
  (7) Install the bolts to the transaxle case and clutch housing as shown in the figure.

Front side fixing bolts

  Tightening torque
  23.6-35.2 N·m
  {2.5-3.5 kgf·m, 17.5-25.9 ft·lbf}

Rear side fixing bolts

  Tightening torque
  23.6-35.2 N·m
  {2.5-3.5 kgf·m, 17.5-25.9 ft·lbf}

33. Install the new sealing caps.

34. Install the reverse idler shaft retaining bolt with new packing.

  Tightening torque
  69.6-90.4 N·m
  {7.1-9.2 kgf·m, 51.4-66.6 ft·lbf}

35. Apply a coat of silicone sealant to the contact surface of the shift control case and the transaxle case.

36. Install the select lever set and the shift component to the transaxle case.

  Caution

  • Apply grease to the positions shown in the figure.

  Caution

  • Be aware that the stem lengths of bolt A and B shown in the figure are different.

  Tightening torque
  14.9-22.3 N·m
  {1.6-2.2 kgf·m, 11.0-16.4 ft·lbf}

37. Install the neutral switch and back-up light switch with new packing.

  Tightening torque
  28.2-52.2 N·m
  {2.9-5.3 kgf·m, 20.8-38.5 ft·lbf}

38. Install a new straight pin.

  Tightening torque
  21.0-39.0 N·m
  {2.2-3.9 kgf·m, 15.5-28.7 ft·lbf}

39. Install a new shift push pin.

  Tightening torque
  20.6-38.2 N·m
  {2.1-3.8 kgf·m, 15.2-28.1 ft·lbf}

40. Install a new select push pin.

  Tightening torque
  27.5-50.9 N·m
  {2.9-5.1 kgf·m, 20.3-37.5 ft·lbf}

41. Install new packing, a drain plug, and a oil level plug.

  Tightening torque
  27.5-50.9 N·m
  {2.9-5.1 kgf·m, 20.3-37.5 ft·lbf}