#
AIRFLOW MODE CONTROL OPERATION

id074000102900

## Airflow Mode Automatic Control

• The climate control unit uses the present opening angle of the air mix actuator and the control condition of the A/C compressor to determine the airflow mode. When the A/C compressor is in OFF mode, the climate control unit varies the determined value of airflow mode according to the temperature signals received from the evaporator temperature sensor.

.

1 | Airflow mode (A/C on mode)
2 | Airflow mode (A/C off mode)
3 | VENT
4 | BI-LEVEL
5 | HEAT
6 | Air mix actuator
7 | COLD
8 | HOT
9 | Amount varies

### Correction

Ambient temperature correction (European (L.H.D. U.K.) specs.)

  • To improve windshield and front door glass from fogging, airflow mode is fixed at HEAT/DEF when the ambient temperature is low. However, ambient temperature correction does not operate when the temperature is set at MAX COLD. (temperature setting dial is turned to the left)

Engine coolant temperature correction (Warm-up correction)

  • Switches the airflow mode after the engine is started in winter in accordance with the increase in engine coolant temperature to prevent discomfort caused by cold air blown towards the feet. The engine coolant temperature correction is performed only when the cabin temperature is 13 °C {55 °F} or less, or the cabin temperature is 23 °C {73 °F} or less and sunlight intensity is relatively low.

1 | DEFROSTER
2 | HEAT/DEF
3 | HEAT
4 | AUTO
5 | LOW
6 | HIGH
7 | Engine coolant temperature

Fail-safe function

  • When the potentiometer of airflow mode actuator is malfunctioning, the airflow mode door is fixed. Under this situation, if the ignition switch is turned to the ON/LOCK position, the airflow mode door is controlled to be fully opened (DEFROSTER) or closed (VENT) based on the ambient temperature. In addition, the door is fully closed (VENT) in the manual VENT, and fully opened (DEFROSTER) in the manual DEFROSTER.

.

1 | Ambient temperature
2 | VENT
3 | DEFROSTER

  • If the airflow mode doors are locked and the target airflow mode is set by the climate control unit which does not reach to within 9 s, the airflow mode actuator drive signal will be stopped to prevent the motor from burning.

## Airflow Mode Manual Control

• Airflow can be selected by operating the MODE switch and the DEFROSTER switch.

Airflow mode | Switch operation | Air outlet
--- | --- | ---
VENT | MODE switch set from HEAT/DEF to VENT | CENTER VENT, SIDE VENT
BI-LEVEL | MODE switch set from VENT to BI-LEVEL | CENTER VENT, SIDE VENT, HEAT
HEAT | MODE switch set from BI-LEVEL to HEAT MODE switch set from DEFROSTER to HEAT | SIDE VENT (L.H.D. only), HEAT, REAR HEAT (minimum air from DEFROSTER and SIDE DEMISTER)
HEAT/DEF | MODE switch set from HEAT to HEAT/DEF | SIDE VENT (L.H.D. only), HEAT, REAR HEAT, DEFROSTER, SIDE DEMISTER
DEFROSTER | DEFROSTER switch to ON | SIDE VENT (L.H.D. only), DEFROSTER, SIDE DEMISTER